{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":7,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-A8"]
[]
[]
[]
[]
["","","","","","2MXM50A2V1B8","2MXM68A2V1B8"]
["Dimensions","Unit","","Height","mm","552","734"]
["","","","Width","mm","852","974"]
["","","","Depth","mm","350","408"]
["Weight","Unit","","","kg","41","60"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","50","50"]
["Sound pressure level","Cooling","","Nom.","dBA","48","48"]
["","Heating","","Nom.","dBA","50","48"]
["Refrigerant","Type","","","","R-32","R-32"]
["","Charge","","","kg","1.15","2.00"]
["","Charge","","","tCO2Eq","0.78","1.35"]
["","GWP","","","","675","675"]
["Piping connections","Piping length","OU - IU","Max.","m","20 (1)","25 (1)"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 20m)","0.02 (for piping length exceeding 30m)"]
["","Level difference","IU - OU","Max.","m","15","15"]
["","","IU - IU","Max.","m","7.5","7.5"]
["","Total piping length","System","Actual","m","30","50"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Drain cap","","","","","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Energy Efficiency Range","","","","","A+++ ~ D","A+++ ~ D"]
["Power supply","Phase","","","","1~","1~"]
["","Frequency","","","Hz","50","50"]
["","Voltage","","","V","220-240","220-240"]
["Notes","","","","","(1) - For one room","(1) - For one room"]
["","","","","","(2) - For combination with CVXM-A, FVXM-A - maximum piping length is 30m.","(2) - For combination with CVXM-A, FVXM-A - maximum piping length is 30m."]
["","","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]
["","","","","","(5) - Contains fluorinated greenhouse gases","(5) - Contains fluorinated greenhouse gases"]