{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":9,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXS-H"]
[]
[]
[]
[]
["","","","","","2MXS40H3V1B","2MXS40H2V1B","2MXS50H3V1B","2MXS50H2V1B"]
["Sound pressure level","Heating","","Nom.","dBA","48","","50"]
["","Cooling","","Nom.","dBA","47","","48"]
["Standard Accessories","Installation manual","","","","1","1","1","1"]
["","Screw bag","","","","1","1","1","1"]
["","Drain plug","","","","1","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","2.5","","3.3"]
["","GWP","","","","2,087.5","","2,087.5"]
["","Charge","","","kg","1.20","","1.60"]
["","Type","","","","R-410A","","R-410A"]
["Piping connections","Level difference","IU - IU","Max.","m","7.5","","7.5"]
["","","IU - OU","Max.","m","15","","15"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 20m)","","0.02 (for piping length exceeding 20m)"]
["","Total piping length","System","Actual","m","30","","30"]
["Dimensions","Unit","","Width","mm","765","","765"]
["","","","Depth","mm","285","","285"]
["","","","Height","mm","550","","550"]
["Compressor","Type","","","","Hermetically sealed swing compressor","","Hermetically sealed swing compressor"]
["Weight","Unit","","","kg","38","","42"]
["Power supply","Phase","","","","1~","","1~"]
["","Frequency","","","Hz","50","","50"]
["","Voltage","","","V","220-240","","220-240"]
["Notes","","","","","(1) - Contains fluorinated greenhouse gases","","(1) - Contains fluorinated greenhouse gases"]
["Dimensions","Unit","","Height","mm","","550","","550"]
["","","","Width","mm","","765","","765"]
["","","","Depth","mm","","285","","285"]
["Weight","Unit","","","kg","","38","","42"]
["Compressor","Type","","","","","Hermetically sealed swing compressor","","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","","10","","10"]
["","","","Max.","°CDB","","46","","46"]
["","Heating","Ambient","Min.","°CWB","","-15","","-15"]
["","","","Max.","°CWB","","15.5","","15.5"]
["Sound pressure level","Cooling","","Nom.","dBA","","47","","48"]
["","Heating","","Nom.","dBA","","48","","50"]
["Refrigerant","Type","","","","","R-410A","","R-410A"]
["","Charge","","","kg","","1.20","","1.60"]
["","Charge","","","tCO2Eq","","2.5","","3.3"]
["","GWP","","","","","2087.5","","2087.5"]
["Piping connections","Piping length","OU - IU","Max.","m","","20","","20"]
["","Additional refrigerant charge","","","kg/m","","0.02 (for piping length exceeding 20m)","","0.02 (for piping length exceeding 20m)"]
["","Level difference","IU - OU","Max.","m","","15","","15"]
["","","IU - IU","Max.","m","","7.5","","7.5"]
["","Total piping length","System","Actual","m","","30","","30"]
["Power supply","Phase","","","","","1~","","1~"]
["","Frequency","","","Hz","","50","","50"]
["","Voltage","","","V","","220-240","","220-240"]
["Standard Accessories","Reducer assembly","","","","","","1","1"]