{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3AMXM-M"]
[]
[]
[]
[]
["","","","","","3AMXM52M3V1B","3AMXM52M2V1B"]
["Sound pressure level","Heating","","Nom.","dBA","47"]
["","Cooling","","Nom.","dBA","46"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Screw bag","","","","1","1"]
["","Drain plug","","","","1","1"]
["","Drain cap (1)","","","","6"]
["","Drain cap (2)","","","","3"]
["","Peel off F-gas label","","","","1"]
["","Additional refrigerant label","","","","1"]
["Refrigerant","Charge","","","TCO2Eq","1.2"]
["","GWP","","","","675"]
["","Charge","","","kg","1.8"]
["","Type","","","","R-32"]
["Fan motor","Speed","Cooling","Super low","rpm","420"]
["","","Heating","Super low","rpm","420"]
["Piping connections","Level difference","IU - IU","Max.","m","7.5"]
["","","IU - OU","Max.","m","15"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 30m)"]
["","Total piping length","System","Actual","m","50"]
["Dimensions","Unit","","Width","mm","868"]
["","","","Depth","mm","320"]
["","","","Height","mm","734"]
["Compressor","Type","","","","Hermetically sealed swing compressor"]
["Weight","Unit","","","kg","57"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]
["Notes","","","","","(1) - Contains fluorinated greenhouse gases"]
["","","","","","(2) - See separate drawing for operation range"]
["","","","","","(3) - See separate drawing for electrical data"]
["Fan","Air flow rate","Cooling","Super low","m³/min","","24"]
["","","Heating","Super low","m³/min","","24"]
["","","","Super low","cfm","","847"]
["","","Heating","Super low","cfm","","847"]
["Dimensions","Unit","","Height","mm","","734"]
["","","","Width","mm","","868"]
["","","","Depth","mm","","320"]
["Weight","Unit","","","kg","","57"]
["Fan motor","Speed","Cooling","Super low","rpm","","420"]
["","","Heating","Super low","rpm","","420"]
["Compressor","Type","","","","","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","","-10"]
["","","","Max.","°CDB","","46"]
["","Heating","Ambient","Min.","°CWB","","-15"]
["","","","Max.","°CWB","","18"]
["Sound pressure level","Cooling","","Nom.","dBA","","46"]
["","Heating","","Nom.","dBA","","47"]
["Refrigerant","Type","","","","","R-32"]
["","Charge","","","kg","","1.80"]
["","Charge","","","tCO2Eq","","1.2"]
["","GWP","","","","","675"]
["Piping connections","Piping length","OU - IU","Max.","m","","25"]
["","Additional refrigerant charge","","","kg/m","","0.02 (for piping length exceeding 30m)"]
["","Level difference","IU - OU","Max.","m","","15"]
["","","IU - IU","Max.","m","","7.5"]
["","Total piping length","System","Actual","m","","50"]
["Power supply","Phase","","","","","1~"]
["","Frequency","","","Hz","","50"]
["","Voltage","","","V","","220-240"]