{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-M / ARXP-M"]
[]
[]
[]
[]
["","","","","ATXP20M5V1B / ARXP20M5V1B","ATXP25M5V1B / ARXP25M5V1B","ATXP35M5V1B / ARXP35M5V1B"]
["Cooling capacity","Min.","","kW","1.3","1.3","1.3"]
["","Nom.","","kW","2.00","2.50","3.50"]
["","Max.","","kW","2.6","3.0","4.0"]
["Heating capacity","Min.","","kW","1.30","1.30","1.30"]
["","Nom.","","kW","2.50","3.00","4.00"]
["","Max.","","kW","3.50","4.00","4.80"]
["Nominal efficiency","COP","","","4.77","4.36","4.02"]
["","EER","","","3.98","3.79","3.45"]
["","Energy labeling Directive","Cooling","","A","A","A"]
["","","Heating","","A","A","A"]
["Space cooling","Annual energy consumption","","kWh/a","104","128","187"]
["","Energy efficiency class","","","A++","A++","A++"]
["","Capacity","Pdesign","kW","2.00","2.50","3.50"]
["","SEER","","","6.77","6.85","6.56"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","663","730","847"]
["","Capacity","Pdesign","kW","2.20","2.40","2.80"]
["","Energy efficiency class","","","A++","A++","A++"]
["","Pdh Heating capacity at -10°","","kW","1.98","2.09","2.32"]
["","SCOP/A","","","4.64","4.60","4.62"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data"]