{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":6,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHH2E-AV3"]
[]
[]
[]
[]
["","","","","","EKHH2E260AAV3"]
["Sound power level","Domestic hot water heating","","Indoor unit","dBA","53"]
["","","","Outdoor unit","dBA","52"]
["Equivalent hot water","Max","","","l","342"]
["Heat pump","Automatic defrost start","","","°C","-2"]
["","Operation range","Ambient","Min.","°CDB","-7"]
["","","","Max.","°CDB","38"]
["","Casing","","Material","","Cover: EPP top finishing"]
["","","","Colour","","White body / black top"]
["","System pressure","","Max.","bar","7"]
["","Defrost method","","","","Active with hot gas valve"]
["Domestic hot water heating","General","","Water heating energy efficiency class","","A+"]
["","","","Thermostat temperature setting","°C","55"]
["","","","Declared load profile","","XL"]
["","Cold climate","","AEC (Annual electricity consumption)","kWh","1,826"]
["","Warm climate","","AEC (Annual electricity consumption)","kWh","1,296"]
["","Average climate","","AEC (Annual electricity consumption)","kWh","1,323"]
["COP","","","","","3.10 (1), 3.60 (2)"]
["Refrigerant","GWP","","","","1,430.0"]
["","Charge","","","kg","0.900"]
["","Type","","","","R-134a"]
["Dimensions","Unit","","Diameter","mm","650"]
["","","","Height","mm","2,000"]
["Compressor","Type","","","","Rotary non-inverter"]
["Domestic hot water","Output","","Nom","kW","1.8"]
["Tank","Installation","","Solar thermal connection possible","","No"]
["","Integrated heating element power","","Nom.","kW","1.5"]
["","Casing","","Material","","Embossed ABS"]
["","","","Colour","","White"]
["","Dimensions","Unit","Height","mm","1,500"]
["","Operation range","Water side","Max.","°C","56"]
["","","","Min.","°C","10"]
["Weight","Packed unit","","","kg","115"]
["","Unit","","Empty","kg","95"]
["","","","Full","kg","349"]
["Installation place","","","","","Indoor"]
["IP class","","","","","IP-X4"]
["General","Product description","","Air-to-water heat pump","","Yes"]
["","Supplier/Manufacturer details","","Name and address","","ELIC - Via Pietro Zorutti 13/14, 33074 Fontanafredda ITALY"]
["Heat up time","Max.","","","hh:mm","10:14:00, 07:56:46"]
["Heat pump","Power supply","","Frequency","Hz","50"]
["","","","Maximum running current","A","2"]
["","","","Phase","","1P"]
["","","","Voltage","V","230"]
["Tank","Power supply","","Phase","","1P"]
["","","","Frequency","Hz","50"]
["","","","Voltage","V","230"]
["Notes","","","","","(1) - According to EN16147-2011, inlet temperature 7°C, room temperature 20°C, cold water inlet 10°C"]
["","","","","","(2) - According to EN16147-2011, inlet temperature 15°C, room temperature 20°C, cold water inlet 10°C"]
["","","","","","(3) - Indoor temperature : 29°CDB, 19°CWB; outdoor temperature : 46°CDB, 24°CWB"]
["","","","","","(4) - Indoor temperature : 27°CDB, 19°CWB; outdoor temperature : 35°CDB, 24°CWB"]