{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":11,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETBH12E9W / EPRA08-12EW"]
[]
[]
[]
[]
["","","","","","ETBH12EF9W / EPRA08EAW1","ETBH12EJ9W / EPRA08EAW1","ETBH12EF9W / EPRA10EAW1","ETBH12EJ9W / EPRA10EAW1","ETBH12EF9W / EPRA12EAW1","ETBH12EJ9W / EPRA12EAW1"]
["Indoor unit","","","","","ETBH12EF9W","","ETBH12EF9W","","ETBH12EF9W"]
["Heating capacity","Min.","","","kW","3.44 (1)","3.44 (1)","3.44 (1)","3.44 (1)","3.44 (1)","3.44 (1)"]
["","Nom.","","","kW","6.17 (2)","6.17 (2)","6.17 (2)","6.17 (2)","6.17 (2)","6.17 (2)"]
["","Max.","","","kW","7.95 (1)","7.95 (1)","9.25 (1)","9.25 (1)","9.97 (1)","9.97 (1)"]
["Power input","Heating","","Min.","kW","0.70 (5)","0.70 (5)","0.70 (5)","0.70 (5)","0.70 (5)","0.70 (5)"]
["","","","Nom.","kW","1.21 (2)","1.21 (2)","1.21 (2)","1.21 (2)","1.21 (2)","1.21 (2)"]
["","","","Max.","kW","1.63 (5)","1.63 (5)","1.98 (5)","1.98 (5)","2.21 (5)","2.21 (5)"]
["COP","","","","","5.10 (2)","5.10 (2)","5.10 (2)","5.10 (2)","5.10 (2)","5.10 (2)"]
["Space heating","Average climate water outlet 55°C","General","SCOP","","3.52","3.52","3.53","3.53","3.53","3.53"]
["","","","Seasonal space heating eff. class","","A++","A++","A++","A++","A++","A++"]
["","Average climate water outlet 35°C","General","SCOP","","4.81","4.81","4.84","4.84","4.84","4.84"]
["","","","Seasonal space heating eff. class","","A+++","A+++","A+++","A+++","A+++","A+++"]
["Energy Efficiency Range","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Notes","","","","","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C","(1) - Capacity according to standard EN14511 and valid for heated water range dT = 3~8°C at Ta 7°C"]
["","","","","","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(2) - Condition: Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(3) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(3) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(3) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(3) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(3) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511","(3) - Power input is total input of indoor and outdoor units, including the circulation pump; according to EN14511"]
["","","","","","(4) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(4) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(4) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(4) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(4) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed","(4) - DB/WB 7°C/6°C - LWC 35°C (dT=5°C) with pump at full speed"]