{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-A / AZAS-MV1"]
[]
[]
[]
[]
["","","","","FAA100AUVEB / AZAS100M7V1B","FAA71AUVEB / AZAS71M2V1B (Archived)"]
["Cooling capacity","Nom.","","kW","9.50 (1)","6.80 (1)"]
["Space cooling","SEER","","","5.25","5.77"]
["","Annual energy consumption","","kWh/a","633","412"]
["","Capacity","Pdesign","kW","9.50","6.80"]
["","Energy efficiency class","","","A","A+"]
["Space heating (Average climate)","Capacity","Pdesign","kW","6.00","4.50"]
["","SCOP/A","","","3.81","3.81"]
["","Energy efficiency class","","","A","A"]
["","Annual energy consumption","","kWh/a","2,205","1,654"]
["Heating capacity","Nom.","","kW","10.8 (2)","7.50 (2)"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]