{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":8,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FAA71BUV1B / RZQG71L9V1B","FAA100BUV1B / RZQG71L9V1B","FAA71BUV1B / FAA71BUV1B / RZQG100L9V1B","FAA100BUV1B / RZQG100L9V1B"]
["Cooling capacity","Nom.","","kW","6.80","6.80","9.50","9.50"]
["Space cooling","SEER","","","6.43","6.43","5.10","6.11"]
["","Annual energy consumption","","kWh/a","371","371","652","545"]
["","Capacity","Pdesign","kW","6.80","6.80","9.50","9.50"]
["","Energy efficiency class","","","A++","A++","A","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","6.33","6.33","11.30","10.20"]
["","SCOP/A","","","4.02","4.02","3.80","4.01"]
["","Energy efficiency class","","","A+","A+","A","A+"]
["","Annual energy consumption","","kWh/a","2,205","2,205","4,164","3,562"]
["Nominal efficiency","EER","","","3.40","3.40","3.75","3.62"]
["","Annual energy consumption","","kWh","1,000","","","1,312"]
["","COP","","","3.70","","","3.61"]
["","Energy labeling Directive","Cooling","","A","","","A"]
["","","Heating","","A","","","A"]
["Heating capacity","Nom.","","kW","7.50","","","10.80"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","","","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","","","(4) - See separate drawing for electrical data"]