{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":8,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / AZAS-MV1"]
[]
[]
[]
[]
["","","","","FCAG71AVEB / AZAS71M2V1B","FCAG100AVEB / AZAS100M7V1B","FCAG125AVEB / AZAS125M7V1B","FCAG140AVEB / AZAS140M7V1B"]
["Cooling capacity","Nom.","","kW","6.80 (1)","","12.1 (1)","13.4 (1)"]
["Heating capacity","Nom.","","kW","7.50 (2)","","13.5 (2)","15.5 (2)"]
["Space cooling","Energy efficiency class","","","A+"]
["","Capacity","Pdesign","kW","6.80","","12.1","13.0"]
["","SEER","","","5.87","","5.40","6.00"]
["","Annual energy consumption","","kWh/a","405","","1,345","1,300"]
["Space heating (Average climate)","Energy efficiency class","","","A"]
["","Capacity","Pdesign","kW","4.50","","6.00","7.80"]
["","SCOP/A","","","4.00","","3.80","4.31"]
["","Annual energy consumption","","kWh/a","1,575","","2,211","2,534"]
["Notes","","","","(1) - Cooling: T2: indoor temp. 26,6°CDB, 19,4°CWB, outdoor temp. 48°CDB [Btu/hr/W]","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB; equivalent piping length: 5m; level difference: 0m"]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["Outdoor unit","","","","","AZAS100M7V1B"]
["Cooling capacity","Nom.","","kW","","9.50 (1)"]
["Heating capacity","Nom.","","kW","","10.8 (2)"]
["Space cooling","Energy efficiency class","","","","A+"]
["","Capacity","Pdesign","kW","","9.50"]
["","SEER","","","","5.67"]
["","Annual energy consumption","","kWh/a","","586"]
["Space heating (Average climate)","Energy efficiency class","","","","A"]
["","Capacity","Pdesign","kW","","6.00"]
["","SCOP/A","","","","3.85"]
["","Annual energy consumption","","kWh/a","","2182"]
["Energy Efficiency Range","","","","","A+++ ~ D"]