{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RXS-L"]
[]
[]
[]
[]
["","","","","FCAG50AVEB / RXS50L2V1B","FCAG60AVEB / RXS60L2V1B"]
["Cooling capacity","Nom.","","kW","5.00","5.70"]
["Space cooling","SEER","","","6.48","6.22"]
["","Annual energy consumption","","kWh/a","270","321"]
["","Capacity","Pdesign","kW","5.00","5.70"]
["","Energy efficiency class","","","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.36","4.71"]
["","SCOP/A","","","4.29","4.00"]
["","Energy efficiency class","","","A++","A+"]
["","Annual energy consumption","","kWh/a","1,426","1,646"]
["Piping connections","Liquid","OD","mm","6.35","6.35"]
["","Gas","OD","mm","12.70","12.70"]
["","Drain","OD","mm","VP25 (External dia.32, internal dia. 25)","VP25 (External dia.32, internal dia. 25)"]
["Nominal efficiency","EER","","","3.55","3.48"]
["","Annual energy consumption","","kWh","705","820"]
["","COP","","","3.70","3.52"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","A","B"]
["Heating capacity","Nom.","","kW","6.00","7.00"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]