{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RXM-A9"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B9 / RXM25A5V1B9","FDXM35F3V1B9 / RXM35A5V1B9"]
["Cooling capacity","Min.","","kW","1.3","1.4"]
["","Nom.","","kW","2.4","3.4"]
["","Max.","","kW","3","3.8"]
["Heating capacity","Min.","","kW","1.3","1.4"]
["","Nom.","","kW","3.2","4"]
["","Max.","","kW","4.5","5"]
["Nominal efficiency","EER","","","3.77","2.98"]
["","COP","","","4","3.48"]
["","Annual energy consumption","","kWh","318","570"]
["","Energy labeling Directive","Cooling","","A","C"]
["","","Heating","","A","B"]
["Space cooling","Energy efficiency class","","","A+","A"]
["","Capacity","Pdesign","kW","2.4","3.4"]
["","SEER","","","5.79","5.35"]
["","Annual energy consumption","","kWh/a","145","222"]
["Space heating (Average climate)","Energy efficiency class","","","A+","A"]
["","Capacity","Pdesign","kW","2.6","2.9"]
["","SCOP/A","","","4.29","3.95"]
["","Pdh Heating capacity at -10°","","kW","2.15","2.32"]
["","Annual energy consumption","","kWh/a","848","1028"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D"]
["Notes","","","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range"]
["","","","","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data"]
["","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]