{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":14,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / RZQG71L8Y1B","FDXM35F3V1B9 / FDXM35F3V1B9 / RZQG71L8Y1B","FDXM50F3V1B9 / FDXM50F3V1B9 / RZQG71L8Y1B","FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / RZQG100L8Y1B","FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / RZQG100L8Y1B","FDXM50F3V1B9 / FDXM50F3V1B9 / FDXM50F3V1B9 / RZQG100L8Y1B","FDXM50F3V1B9 / FDXM50F3V1B9 / RZQG100L8Y1B","FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / RZQG125L8Y1B","FDXM50F3V1B9 / FDXM50F3V1B9 / FDXM50F3V1B9 / RZQG125L8Y1B","FDXM60F3V1B9 / FDXM60F3V1B9 / RZQG125L8Y1B"]
["Cooling capacity","Nom.","","kW","6.80","6.80","6.80","9.50","9.50","9.50","9.50","12.00","12.00","12.00"]
["Space cooling","SEER","","","4.80","4.80","4.80","5.10","5.10","5.10","5.10","5.10","5.10","5.10"]
["","Annual energy consumption","","kWh/a","496","496","496","652","652","652","652","824","824","824"]
["","Capacity","Pdesign","kW","6.80","6.80","6.80","9.50","9.50","9.50","9.50","12.00","12.00","12.00"]
["","Energy efficiency class","","","B","B","B","A","A","A","A","A","A","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","6.00","6.00","6.00","10.74","10.74","11.30","11.30","11.30","12.71","12.71"]
["","SCOP/A","","","3.80","3.80","3.80","3.80","3.80","3.80","3.80","3.80","3.80","3.80"]
["","Energy efficiency class","","","A","A","A","A","A","A","A","A","A","A"]
["","Annual energy consumption","","kWh/a","2,211","2,211","2,211","3,957","3,957","4,164","4,164","4,164","4,683","4,683"]
["Nominal efficiency","EER","","","3.06","3.06","3.06","3.38","3.38","3.78","3.78","3.05","3.48","3.20"]
["Notes","","","","(1) - See separate drawing for operation range","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - See separate drawing for operation range","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - See separate drawing for electrical data","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - See separate drawing for electrical data","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","(3) - See separate drawing for operation range","","","(3) - See separate drawing for operation range","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","","(4) - See separate drawing for electrical data","","","(4) - See separate drawing for electrical data","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]