{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F"]
[]
[]
[]
[]
["","","","","FDXS25F2VEB","FDXS35F2VEB","FDXS60F2VEB"]
["Sound pressure level","Heating","High","dBA","35","35","38"]
["","","Medium","dBA","33","33","36"]
["","","Low","dBA","27","27","30"]
["","Cooling","Medium","dBA","33","33","35"]
["","","Low","dBA","27","27","30"]
["","","High","dBA","35","35","38"]
["Standard Accessories","Installation manual","","","1","1","1"]
["","Operation manual","","","1","1","1"]
["","Insulation for fitting","","","1","1","1"]
["","Sealing pad","","","1","1","1"]
["","Clamp metal","","","1","1","1"]
["","Drain hose","","","1","1","1"]
["","Washer for hanger bracket","","","8","8","8"]
["","Sealing material","","","2","2","2"]
["","Clamps","","","6","6","6"]
["","Washer fixing plate","","","4","4","4"]
["","Screws for duct flanges","","","1","1","1"]
["","Air filter","","","1","1","1"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35"]
["","Gas","OD","mm","9.50","9.50","12.7"]
["","Drain","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Power input","Cooling","Nom.","kW","0.036","0.036","0.060"]
["","Heating","Nom.","kW","0.036","0.036","0.060"]
["Sound power level","Cooling","","dBA","53","53","56"]
["","Heating","","dBA","53","53","56"]
["Dimensions","Unit","Width","mm","750","750","1,150"]
["","","Depth","mm","620","620","620"]
["","","Height","mm","200","200","200"]
["Weight","Unit","","kg","21.0","21.0","30.0"]
["Fan","External static pressure","Nom.","Pa","30","30","40"]
["Power supply","Phase","","","1~","1~","1~"]
["","Name","","","VE","VE","VE"]
["","Frequency","","Hz","50/60","50/60","50/60"]
["","Voltage","","V","220-240","220-240","220-240"]
["Notes","","","","(1) - Operating sound is based on the rear side suction inlet and ESP 40Pa. Operating sound for under side suction inlet: (operation sound for rear side suction inlet) +5dB. However, when installation to which the ESP becomes low is carried out, 5dB or more may","(1) - Operating sound is based on the rear side suction inlet and ESP 40Pa. Operating sound for under side suction inlet: (operation sound for rear side suction inlet) +5dB. However, when installation to which the ESP becomes low is carried out, 5dB or more may","(1) - Operating sound is based on the rear side suction inlet and ESP 40Pa. Operating sound for under side suction inlet: (operation sound for rear side suction inlet) +5dB. However, when installation to which the ESP becomes low is carried out, 5dB or more may"]
["","","","","(2) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected.","(2) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected.","(2) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected."]