{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":8,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FHQ100CAVEB / RZQG71L9V1B","FHQ71CAVEB / RZQG71L9V1B","FHQ100CAVEB / RZQG100L9V1B","FHQ125CAVEB / RZQG125L9V1B"]
["Cooling capacity","Nom.","","kW","","6.8","9.5","12.0"]
["Space cooling","SEER","","","6.95","6.95","6.11","6.01"]
["","Annual energy consumption","","kWh/a","343","343","545","699"]
["","Capacity","Pdesign","kW","6.80","6.80","9.50","12.00"]
["","Energy efficiency class","","","A++","A++","A++","A+"]
["Space heating (Average climate)","Capacity","Pdesign","kW","7.60","7.60","11.30","14.13"]
["","SCOP/A","","","4.32","4.32","4.61","4.23"]
["","Energy efficiency class","","","A+","A+","A++","A+"]
["","Annual energy consumption","","kWh/a","2,463","2,463","3,432","4,677"]
["Nominal efficiency","EER","","","","3.82","3.81","3.35"]
["","Annual energy consumption","","kWh","","890","1,245","1,790"]
["","COP","","","","4.13","4.15","3.89"]
["","Energy labeling Directive","Cooling","","","A","A","A"]
["","","Heating","","","A","A","A"]
["Heating capacity","Nom.","","kW","","7.5","10.8","13.5"]
["Notes","","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]