{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":7,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-A / RXM-A"]
[]
[]
[]
[]
["","","","","FTXM25A5V1B / RXM25A5V1B","FTXM35A2V1B / RXM35A5V1B","FTXM42A5V1B / RXM42A5V1B"]
["Cooling capacity","Min.","","kW","0.90","0.90","1.50"]
["","Nom.","","kW","2.50","3.50","4.20"]
["","Max.","","kW","3.80","4.40","5.20"]
["Heating capacity","Min.","","kW","0.80","0.80","1.50"]
["","Nom.","","kW","2.80","4.00","5.40"]
["","Max.","","kW","5.00","5.50","6.20"]
["Nominal efficiency","EER","","","5.20","4.63","4.20"]
["","COP","","","5.00","4.55","4.19"]
["","Annual energy consumption","","kWh","240","378","500"]
["","Energy labeling Directive","Cooling","","A","A","A"]
["","","Heating","","A","A","A"]
["Space cooling","Energy efficiency class","","","A+++","A+++","A++"]
["","Capacity","Pdesign","kW","2.50","3.50","4.20"]
["","SEER","","","9.47","9.25","8.11"]
["","Annual energy consumption","","kWh/a","92","132","181"]
["Space heating (Average climate)","Energy efficiency class","","","A+++","A+++","A++"]
["","Capacity","Pdesign","kW","2.40","2.50","4.00"]
["","SCOP/A","","","5.20","5.20","5.00"]
["","Pdh Heating capacity at -10°","","kW","2.40","2.50","4.00"]
["","Annual energy consumption","","kWh/a","647","673","1120"]