{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":26,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R / 2MXM-A9"]
[]
[]
[]
[]
["","","","","FTXM20R2V1B / FTXM25R2V1B / 2MXM40A2V1B9","FTXM20R2V1B / FTXM35R2V1B / 2MXM40A2V1B9","FTXM20R5V1B / FTXM35R5V1B / 2MXM40A2V1B9","FTXM25R5V1B / FTXM35R5V1B / 2MXM40A2V1B9","FTXM25R5V1B / FTXM25R5V1B / 2MXM40A2V1B9","FTXM20R2V1B / FTXM20R2V1B / 2MXM40A2V1B9","FTXM20R5V1B / FTXM20R5V1B / 2MXM40A2V1B9","FTXM35R2V1B / FTXM50R2V1B / 2MXM50A2V1B9","FTXM25R2V1B / FTXM42R2V1B / 2MXM50A2V1B9","FTXM35R2V1B / FTXM35R2V1B / 2MXM50A2V1B9","FTXM35R2V1B / FTXM42R2V1B / 2MXM50A2V1B9","FTXM20R2V1B / FTXM42R2V1B / 2MXM50A2V1B9","FTXM25R2V1B / FTXM35R2V1B / 2MXM50A2V1B9","FTXM25R5V1B / FTXM35R5V1B / 2MXM50A2V1B9","FTXM25R5V1B / FTXM42R5V1B / 2MXM50A2V1B9","FTXM35R5V1B / FTXM35R5V1B / 2MXM50A2V1B9","FTXM35R5V1B / FTXM42R5V1B / 2MXM50A2V1B9","FTXM42R5V1B / FTXM42R5V1B / 2MXM50A2V1B9","FTXM20R5V1B / FTXM35R5V1B / 2MXM50A2V1B9","FTXM25R2V1B / FTXM42R2V1B / 2MXM68A2V1B9","FTXM35R5V1B / FTXM35R5V1B / 2MXM68A2V1B9","FTXM25R5V1B / FTXM42R5V1B / 2MXM68A2V1B9"]
["Cooling capacity","Nom.","","kW","4.00","4.00","4.00","4.00","4.00","","","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00"]
["Heating capacity","Nom.","","kW","4.20","4.20","4.20","4.20","4.20","","","5.60","5.60","5.60","5.60","5.60","5.60","5.60","5.60","5.60","5.60","5.60","5.60"]
["Nominal efficiency","Annual energy consumption","","kWh","481","476","476","472","478","","","598","611","608","604","614","616","616","611","608","604","601","619"]
["","COP","","","4.32","4.41","4.41","4.46","4.37","","","3.94","4.03","4.01","4.00","4.13","4.05","4.05","4.03","4.01","4.00","3.98","4.12"]
["","EER","","","4.16","4.20","4.20","4.24","4.18","","","4.18","4.09","4.11","4.14","4.07","4.06","4.06","4.09","4.11","4.14","4.16","4.04"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","","","A","A","A","A","A","A","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","","","A","A","A","A","A","A","A","A","A","A","A","A"]
["Space cooling","Annual energy consumption","","kWh/a","165","171","171","173","168","","","205","204","204","203","205","204","204","204","204","203","204","205"]
["","Energy efficiency class","","","A+++","A++","A++","A++","A++","","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["","Capacity","Pdesign","kW","4.00","4.00","4.00","4.00","4.00","","","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00","5.00"]
["","SEER","","","8.50","8.19","8.19","8.11","8.36","","","8.53","8.58","8.58","8.60","8.54","8.56","8.56","8.58","8.58","8.60","8.57","8.54"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","973","974","974","971","974","","","1,243","1,265","1,269","1,266","1,277","1,272","1,272","1,265","1,269","1,266","1,259","1,275"]
["","Capacity","Pdesign","kW","3.20","3.20","3.20","3.20","3.20","","","4.20","4.20","4.20","4.20","4.20","4.20","4.20","4.20","4.20","4.20","4.20","4.20"]
["","Energy efficiency class","","","A++","A++","A++","A++","A++","","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Pdh Heating capacity at -10°","","kW","2.56","2.58","2.58","2.59","2.57","","","3.25","2.91","2.93","2.95","2.88","2.89","2.89","2.91","2.93","2.95","2.97","2.86"]
["","SCOP/A","","","4.60","4.60","4.60","4.61","4.60","","","4.73","4.65","4.63","4.64","4.61","4.62","4.62","4.65","4.63","4.64","4.67","4.61"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]
["Cooling capacity","Nom.","","kW","","","","","","4","4","","","","","","","","","","","","","6.7","6.8","6.7"]
["Heating capacity","Nom.","","kW","","","","","","4.2","4.2","","","","","","","","","","","","","8.30","8.60","8.30"]
["Nominal efficiency","EER","","","","","","","","4.3","4.3","","","","","","","","","","","","","3.74","3.94","3.74"]
["","COP","","","","","","","","4.28","4.28","","","","","","","","","","","","","3.95","3.81","3.95"]
["","Annual energy consumption","","kWh","","","","","","465","465","","","","","","","","","","","","","896","863","896"]
["","Energy labeling Directive","Cooling","","","","","","","A","A"]
["","","Heating","","","","","","","A","A"]
["Space cooling","Energy efficiency class","","","","","","","","A+++","A+++","","","","","","","","","","","","","A++","A++","A++"]
["","Capacity","Pdesign","kW","","","","","","4","4","","","","","","","","","","","","","6.70","6.80","6.70"]
["","SEER","","","","","","","","8.53","8.53","","","","","","","","","","","","","6.94","6.97","6.94"]
["","Annual energy consumption","","kWh/a","","","","","","164","164","","","","","","","","","","","","","338","342","338"]
["Space heating (Average climate)","Energy efficiency class","","","","","","","","A++","A++","","","","","","","","","","","","","A","A+","A"]
["","Capacity","Pdesign","kW","","","","","","3.2","3.2","","","","","","","","","","","","","4.30","4.80","4.30"]
["","SCOP/A","","","","","","","","4.64","4.64","","","","","","","","","","","","","3.86","4.00","3.86"]
["","Pdh Heating capacity at -10°","","kW","","","","","","2.55","2.55","","","","","","","","","","","","","3.41","3.73","3.41"]
["","Annual energy consumption","","kWh/a","","","","","","966","966","","","","","","","","","","","","","1560","1680","1560"]
["Energy Efficiency Range","","","","","","","","","","","","","","","","","","","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]