{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":24,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R / 4MXM-A"]
[]
[]
[]
[]
["","","","","FTXM20R2V1B / FTXM20R2V1B / FTXM25R2V1B / 4MXM68A2V1B","FTXM20R2V1B / FTXM25R2V1B / FTXM25R2V1B / 4MXM68A2V1B","FTXM20R2V1B / FTXM50R2V1B / 4MXM68A2V1B","FTXM20R5V1B / FTXM20R5V1B / FTXM25R5V1B / 4MXM68A2V1B","FTXM20R5V1B / FTXM25R5V1B / FTXM25R5V1B / 4MXM68A2V1B","FTXM20R5V1B / FTXM50R2V1B / 4MXM68A2V1B","FTXM25R2V1B / FTXM42R2V1B / 4MXM68A2V1B","FTXM25R5V1B / FTXM42R5V1B / 4MXM68A2V1B","FTXM35R2V1B / FTXM35R2V1B / 4MXM68A2V1B","FTXM35R5V1B / FTXM35R5V1B / 4MXM68A2V1B","FTXM20R2V1B / FTXM20R2V1B / FTXM20R2V1B / FTXM20R2V1B / 4MXM80A2V1B","FTXM20R2V1B / FTXM20R2V1B / FTXM42R2V1B / 4MXM80A2V1B","FTXM20R2V1B / FTXM25R2V1B / FTXM35R2V1B / 4MXM80A2V1B","FTXM20R2V1B / FTXM60R2V1B / 4MXM80A2V1B","FTXM20R5V1B / FTXM20R5V1B / FTXM20R5V1B / FTXM20R5V1B / 4MXM80A2V1B","FTXM20R5V1B / FTXM20R5V1B / FTXM42R5V1B / 4MXM80A2V1B","FTXM20R5V1B / FTXM25R5V1B / FTXM35R5V1B / 4MXM80A2V1B","FTXM20R5V1B / FTXM60R2V1B / 4MXM80A2V1B","FTXM35R2V1B / FTXM42R2V1B / 4MXM80A2V1B","FTXM35R5V1B / FTXM42R5V1B / 4MXM80A2V1B"]
["Cooling capacity","Nom.","","kW","6.5","6.8","6.8","6.5","6.8","6.8","6.7","6.7","6.8","6.8","7.40","8.00","7.40","7.40","7.40","8.00","7.40","7.40","7.70","7.70"]
["Space cooling","SEER","","","7.76","7.71","6.75","7.76","7.71","6.75","6.94","6.94","6.97","6.97","7.40","6.93","7.07","6.73","7.40","6.93","7.07","6.73","6.52","6.52"]
["","Annual energy consumption","","kWh/a","294","309","352","294","309","352","338","338","342","342","351","405","370","387","351","405","370","387","417","417"]
["","Capacity","Pdesign","kW","6.50","6.80","6.80","6.50","6.80","6.80","6.70","6.70","6.80","6.80","7.40","8.00","7.40","7.40","7.40","8.00","7.40","7.40","7.70","7.70"]
["","Energy efficiency class","","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","5.30","5.30","4.50","5.30","5.30","4.50","4.30","4.30","4.80","4.80","6.23","5.37","5.37","4.27","6.23","5.37","5.37","4.27","4.27","4.27"]
["","SCOP/A","","","4.09","4.10","3.90","4.09","4.10","3.90","3.86","3.86","4.00","4.00","4.56","4.34","4.31","4.33","4.56","4.34","4.31","4.33","4.23","4.23"]
["","Energy efficiency class","","","A+","A+","A","A+","A+","A","A","A","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+"]
["","Annual energy consumption","","kWh/a","1,814","1,807","1,612","1,814","1,807","1,612","1,559","1,559","1,680","1,680","1,913","1,732","1,744","1,382","1,913","1,732","1,744","1,382","1,413","1,413"]
["Nominal efficiency","EER","","","4.01","3.85","3.59","4.01","3.85","3.59","3.74","3.74","3.94","3.94","4.17","3.56","3.79","3.43","4.17","3.56","3.79","3.43","3.11","3.11"]
["","Annual energy consumption","","kWh","810","883","947","810","883","947","896","896","863","863","887","1,125","977","1,079","887","1,125","977","1,079","1,236","1,236"]
["","COP","","","4.49","4.38","3.82","4.49","4.38","3.82","3.95","3.95","3.81","3.81","4.58","4.08","4.02","3.73","4.58","4.08","4.02","3.73","3.56","3.56"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","B","B"]
["","","Heating","","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","B","B"]
["Heating capacity","Nom.","","kW","8.20","8.60","8.60","8.20","8.60","8.60","8.30","8.30","8.60","8.60","9.60","9.40","9.30","9.30","9.60","9.40","9.30","9.30","9.00","9.00"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]