{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":18,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R / RXM-N9"]
[]
[]
[]
[]
["","","","","FTXM20R5V1B / RXM20N5V1B9","FTXM20R2V1B / RXM20N5V1B9","FTXM20R2V1B / RXM20N2V1B9","FTXM25R2V1B / RXM25N5V1B9","FTXM25R5V1B / RXM25N5V1B9","FTXM25R5V1B / RXM25N2V1B9","FTXM20R5V1B / RXM20N2V1B9","FTXM25R2V1B / RXM25N2V1B9","FTXM35R2V1B / RXM35N5V1B9","FTXM35R5V1B / RXM35N5V1B9","FTXM35R2V1B / RXM35N2V1B9","FTXM35R5V1B / RXM35N2V1B9","FTXM50R2V1B / RXM50N2V1B9","FTXM60R2V1B / RXM60N2V1B9"]
["Outdoor unit","","","","RXM20N5V1B9","RXM20N5V1B9","RXM20N5V1B9","RXM25N5V1B9","RXM25N5V1B9","RXM25N5V1B9","RXM20N5V1B9","RXM25N5V1B9","RXM35N5V1B9","RXM35N5V1B9","RXM35N5V1B9","RXM35N5V1B9","RXM50N2V1B9","RXM60N2V1B9"]
["Cooling capacity","Min.","","kW","1.30","1.30","","1.30","1.30","","","","1.40","1.40","","","1.70","1.70"]
["","Nom.","","kW","2.00","2.00","","2.50","2.50","","","","3.40","3.40","","","5.00","6.00"]
["","Max.","","kW","2.60","2.60","","3.20","3.20","","","","4.00","4.00","","","6.00","7.00"]
["Heating capacity","Min.","","kW","1.30","1.30","","1.30","1.30","","","","1.40","1.40","","","1.70","1.70"]
["","Nom.","","kW","2.50","2.50","","2.80","2.80","","","","4.00","4.00","","","5.80","7.00"]
["","Max.","","kW","3.50","3.50","","4.70","4.70","","","","5.20","5.20","","","7.70","8.00"]
["Nominal efficiency","Annual energy consumption","","kWh","219","219","","278","278","","","","402","402","","","679","885"]
["","COP","","","5.00","5.00","","5.00","5.00","","","","4.04","4.04","","","4.00","3.61"]
["","EER","","","4.57","4.57","","4.50","4.50","","","","4.23","4.23","","","3.68","3.39"]
["","Energy labeling Directive","Cooling","","A","A","","A","A","","","","A","A","","","A","A"]
["","","Heating","","A","A","","A","A","","","","A","A","","","A","A"]
["Space cooling","Annual energy consumption","","kWh/a","81","81","","101","101","","","","138","138","","","236","304"]
["","Energy efficiency class","","","A+++","A+++","","A+++","A+++","","","","A+++","A+++","","","A++","A++"]
["","Capacity","Pdesign","kW","2.00","2.00","","2.50","2.50","","","","3.40","3.40","","","5.00","6.00"]
["","SEER","","","8.65","8.65","","8.65","8.65","","","","8.65","8.65","","","7.41","6.90"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","632","632","","659","659","","","","687","687","","","1,369","1,562"]
["","Capacity","Pdesign","kW","2.30","2.30","","2.40","2.40","","","","2.50","2.50","","","4.60","4.80"]
["","Energy efficiency class","","","A+++","A+++","","A+++","A+++","","","","A+++","A+++","","","A++","A+"]
["","Pdh Heating capacity at -10°","","kW","2.24","2.24","","2.30","2.30","","","","2.35","2.35","","","4.09","4.11"]
["","SCOP/A","","","5.10","5.10","","5.10","5.10","","","","5.10","5.10","","","4.71","4.30"]
["Notes","","","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","","","","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range","(1) - See separate drawing for operation range"]
["","","","","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","","","","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data","(2) - See separate drawing for electrical data"]
["","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","","","","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(3) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","","","","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(4) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["Cooling capacity","Min.","","kW","","","1.30","","","1.30","1.30","1.30","","","1.40","1.40"]
["","Nom.","","kW","","","2.00","","","2.50","2.00","2.50","","","3.40","3.40"]
["","Max.","","kW","","","2.60","","","3.20","2.60","3.20","","","4.00","4.00"]
["Heating capacity","Min.","","kW","","","1.30","","","1.30","1.30","1.30","","","1.40","1.40"]
["","Nom.","","kW","","","2.50","","","2.80","2.50","2.80","","","4.00","4.00"]
["","Max.","","kW","","","3.50","","","4.70","3.50","4.70","","","5.20","5.20"]
["Nominal efficiency","EER","","","","","4.57","","","4.50","4.57","4.50","","","4.23","4.23"]
["","COP","","","","","5.00","","","5.00","5.00","5.00","","","4.04","4.04"]
["","Annual energy consumption","","kWh","","","219","","","278","219","278","","","402","402"]
["","Energy labeling Directive","Cooling","","","","A","","","A","A","A","","","A","A"]
["","","Heating","","","","A","","","A","A","A","","","A","A"]
["Space cooling","Energy efficiency class","","","","","A+++","","","A+++","A+++","A+++","","","A+++","A+++"]
["","Capacity","Pdesign","kW","","","2.00","","","2.50","2.00","2.50","","","3.40","3.40"]
["","SEER","","","","","8.65","","","8.65","8.65","8.65","","","8.65","8.65"]
["","Annual energy consumption","","kWh/a","","","81","","","101","81","101","","","138","138"]
["Space heating (Average climate)","Energy efficiency class","","","","","A+++","","","A+++","A+++","A+++","","","A+++","A+++"]
["","Capacity","Pdesign","kW","","","2.30","","","2.40","2.30","2.40","","","2.50","2.50"]
["","SCOP/A","","","","","5.10","","","5.10","5.10","5.10","","","5.10","5.10"]
["","Pdh Heating capacity at -10°","","kW","","","2.24","","","2.30","2.24","2.30","","","2.35","2.35"]
["","Annual energy consumption","","kWh/a","","","632","","","659","632","659","","","687","687"]
["Energy Efficiency Range","","","","","","A+++ ~ D","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","","","A+++ ~ D","A+++ ~ D"]