{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRYEQ-AY"]
[]
[]
[]
[]
["","","","","","LRYEQ16A7Y1"]
["Standard Accessories","Installation manual","","","","1"]
["","Operation manual","","","","1"]
["","Connection pipes","","","","1"]
["","Refrigerant label for F-gas regulation","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["Compressor 2","Type","","","","Hermetically sealed scroll compressor"]
["Weight","Unit","","","kg","370"]
["Refrigerant","Charge","","","TCO2Eq","24.0"]
["","GWP","","","","2,087.5"]
["","Charge","","","kg","11.5"]
["","Type","","","","R-410A"]
["Fan motor","Output","","","W","750"]
["","Drive","","","","Direct drive"]
["Heat exchanger","Type","","","","Cross fin coil"]
["Dimensions","Unit","","Width","mm","1,240"]
["","","","Depth","mm","765"]
["","","","Height","mm","1,680"]
["Casing","Colour","","","","Ivory white"]
["Fan","Type","","","","Propeller fan"]
["","Quantity","","","","2"]
["","Air flow rate","Cooling","Nom.","m³/min","230"]
["Power supply","Phase","","","","3~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","380-415"]
["Notes","","","","","(1) - Cooling priority mode: indoor temp. 27°CDB, 19°CWB; outdoor temp. 32°CDB; piping length: 7.5m; level difference: 0m"]
["","","","","","(2) - Cooling priority mode: evaporating temp. -10°C; outdoor temp. 32°CDB; Suction SH: 10°C"]
["","","","","","(3) - Heat recovery 100% mode: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; refrigeration load 18kW; piping length: 7.5m; level difference: 0m"]
["","","","","","(4) - Saturated temperature equivalent to suction pressure (refrigeration side): -10°C (under chilled condition); connection capacity for indoor air conditioner: 10HP, when heat recovery is 100%"]
["","","","","","(5) - Compressor 1"]
["","","","","","(6) - Compressor 2"]
["","","","","","(7) - Compressor 3"]
["","","","","","(8) - Factory charge of unit"]
["","","","","","(9) - Install the oil trap per 5m from the outdoor unit"]
["","","","","","(10) - For more details, see operation range drawing"]
["","","","","","(11) - For more details on standard accessories refer to Installation/operation manual"]
["","","","","","(12) - Contains fluorinated greenhouse gases"]