{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":6,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F8"]
[]
[]
[]
[]
["","","","","","RXS71FAV1B8"]
["Fan","Air flow rate","Cooling","Super low","m³/min","46.0"]
["","","Heating","Super low","m³/min","46.0"]
["","","","Super low","cfm","1624"]
["","","Heating","Super low","cfm","1624"]
["Dimensions","Unit","","Height","mm","770"]
["","","","Width","mm","900"]
["","","","Depth","mm","320"]
["Weight","Unit","","","kg","71"]
["Fan motor","Speed","Cooling","Super low","rpm","730"]
["","","Heating","Super low","rpm","730"]
["Compressor","Type","","","","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","-10"]
["","","","Max.","°CDB","46"]
["","Heating","Ambient","Min.","°CWB","-15"]
["","","","Max.","°CWB","18"]
["Sound pressure level","Cooling","","High","dBA","52"]
["","Heating","","High","dBA","52"]
["Refrigerant","Type","","","","R-410A"]
["","Charge","","","kg","2.3"]
["","Charge","","","tCO2Eq","4.8"]
["","GWP","","","","2087.5"]
["Piping connections","Piping length","OU - IU","Max.","m","30"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","m","20"]
["Standard Accessories","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain socket assy","","","","1"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]
["Notes","","","","","(1) - 220V"]
["","","","","","(2) - 230V"]
["","","","","","(3) - 240V"]