{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":57,"n_cols":12,"rows_kept":57,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-K"]
[]
[]
[]
[]
["","","","","","RXS20K3V1B","RXS20K2V1B","RXS25K3V1B","RXS25K2V1B","RXS35K2V1B","RXS42K2V1B","RXS50K2V1B"]
["Sound pressure level","Heating","","High","dBA","47","","47","","48","48","48"]
["","Cooling","","High","dBA","46","","46","","48","48","48"]
["Standard Accessories","Joint (drain)","","","","1","1","1","1"]
["","Installation manual","","","","1","1","1","1","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","2.1","","2.1","","2.5","2.7","3.5"]
["","GWP","","","","2,087.5","","2,087.5","","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","1.0","","1.0","","1.2","1.3","1.7"]
["","Type","","","","R-410A","","R-410A","","R-410A","R-410A","R-410A"]
["Fan motor","Speed","Cooling","Super low","rpm","780","","780","","780","790","670"]
["","","Heating","Super low","rpm","740","","740","","740","780","670"]
["Piping connections","Level difference","IU - OU","Max.","m","15","","15","","15","15","20"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)","","0.02 (for piping length exceeding 10m)","","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["Dimensions","Unit","","Width","mm","765","","765","","765","765","825"]
["","","","Depth","mm","285","","285","","285","285","300"]
["","","","Height","mm","550","","550","","550","550","735"]
["Compressor","Type","","","","Hermetically sealed swing compressor","","Hermetically sealed swing compressor","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Weight","Unit","","","kg","34","","34","","34","39","47"]
["Fan","Air flow rate","Heating","Super low","cfm","","","","","904","960","1,522"]
["","","Cooling","Super low","cfm","","","","","1,063","1,080","1,727"]
["Power supply","Phase","","","","1~","","1~","","1~","1~","1~"]
["","Frequency","","","Hz","50","","50","","50","50","50"]
["","Voltage","","","V","220-240","","220-240","","220-240","220-240","220-240"]
["Notes","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - SL: The silent fan level of the air flow rate setting","","(4) - SL: The silent fan level of the air flow rate setting","","(4) - Contains fluorinated greenhouse gases","(4) - Contains fluorinated greenhouse gases","(4) - Contains fluorinated greenhouse gases"]
["","","","","","(5) - Contains fluorinated greenhouse gases","","(5) - Contains fluorinated greenhouse gases"]
["Dimensions","Unit","","Height","mm","","550","","550"]
["","","","Width","mm","","765","","765"]
["","","","Depth","mm","","285","","285"]
["Weight","Unit","","","kg","","34","","34"]
["Fan motor","Speed","Cooling","Super low","rpm","","780","","780"]
["","","Heating","Super low","rpm","","740","","740"]
["Compressor","Type","","","","","Hermetically sealed swing compressor","","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","","-10","","-10"]
["","","","Max.","°CDB","","46","","46"]
["","Heating","Ambient","Min.","°CWB","","-15","","-15"]
["","","","Max.","°CWB","","18","","18"]
["Sound pressure level","Cooling","","High","dBA","","46","","46"]
["","Heating","","High","dBA","","47","","47"]
["Refrigerant","Type","","","","","R-410A","","R-410A"]
["","Charge","","","kg","","1.0","","1.0"]
["","Charge","","","tCO2Eq","","2.1","","2.1"]
["","GWP","","","","","2087.5","","2087.5"]
["Piping connections","Piping length","OU - IU","Max.","m","","20","","20"]
["","Additional refrigerant charge","","","kg/m","","0.02 (for piping length exceeding 10m)","","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","m","","15","","15"]
["Power supply","Phase","","","","","1~","","1~"]
["","Frequency","","","Hz","","50","","50"]
["","Voltage","","","V","","220-240","","220-240"]
["Standard Accessories","Drain plug","","","","","","","","1","1","1"]