{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-MV1"]
[]
[]
[]
[]
["","","","","","RZAG71M7V1B","RZAG100M7V1B","RZAG125M7V1B"]
["Dimensions","Unit","","Height","mm","990","1430","1430"]
["","","","Width","mm","940","940","940"]
["","","","Depth","mm","320","320","320"]
["Weight","Unit","","","kg","70","92","92"]
["Compressor","Type","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","-20","-20","-20"]
["","","","Max.","°CDB","52","52","52"]
["","Heating","Ambient","Min.","°CWB","-20","-20","-20"]
["","","","Max.","°CWB","18.0","18.0","18.0"]
["Sound power level","Cooling","","","dBA","64","66","69"]
["Sound pressure level","Cooling","","Nom.","dBA","46","47","50"]
["","Heating","","Nom.","dBA","49","51","52"]
["Refrigerant","Type","","","","R-32","R-32","R-32"]
["","Charge","","","kg","2.95","3.75","3.75"]
["","GWP","","","","675","675","675"]
["","Charge","","","tCO2Eq","1.99","2.53","2.53"]
["Piping connections","Liquid","","OD","mm","9.52","9.52","9.52"]
["","Gas","","OD","mm","15.9","15.9","15.9"]
["","Piping length","OU - IU","Max.","m","55","85","85"]
["","","System","Equivalent","m","75","100","100"]
["","","","Chargeless","m","40","40","40"]
["","Additional refrigerant charge","","","kg/m","See installation manual","See installation manual","See installation manual"]
["","Level difference","IU - OU","Max.","m","30.0","30.0","30.0"]
["","","IU - IU","Max.","m","0.5","0.5","0.5"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Tie-wraps","","","","2","2","2"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240"]
["Current - 50Hz","Maximum fuse amps (MFA)","","","A","20","32","32"]
["Sound power level","Heating","","","dBA","","","69 (1)"]
["Notes","","","","","","","(1) - According to ENER Lot 21"]